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EMPO PROPERTY INSPECTION CHECKLIST
HHSRS 2026 Property Condition Assessment Template
Property Address: _______________________________
Inspection Date: _______________________________
Inspector: _______________________________
Tenant Present: YES / NO
Next Inspection Due: _______________________________

SECTION 1
GENERAL PROPERTY CONDITION
	Item
	 Satisfactory
	 Action Required
	 Comments

	Property generally clean and maintained
	 □
	 □ 
	

	Signs of damage or neglect
	 □
	 □
	

	Structural concerns visible
	 □
	 □
	

	External areas safe and accessible
	 □
	 □
	

	Boundaries secure
	 □
	 □
	


Notes:



SECTION 2
HHSRS ACCIDENT HAZARDS
Falls on the Level
	Check
	Yes
	No

	Flooring safe and secure
	□
	□

	No loose carpets
	□
	□

	No uneven flooring
	□
	□

	Walkways clear
	□
	□

	Adequate lighting provided
	□
	□


Stairs and Steps
	Check
	Yes
	No

	Handrails present and secure
	□
	□

	Stair coverings secure
	□
	□

	No damaged steps
	□
	□

	Stair lighting adequate
	□
	□


Falls Between Levels
	Check
	Yes
	No

	Window restrictors fitted where required
	□
	□

	Balustrades secure
	□
	□

	Landings safe
	□
	□


Fire & Explosions
	Check
	Yes
	No

	Smoke alarms operational
	□
	□

	Heat alarms operational
	□
	□

	Escape routes unobstructed
	□
	□

	Fire doors functioning (where applicable)
	□
	□

	No obvious fire risks
	□
	□


Electrical Hazards
	Check
	Yes
	No

	No exposed wiring
	□
	□

	Sockets secure
	□
	□

	Consumer unit appears satisfactory
	□
	□

	No overloaded extension leads
	□
	□


Structural Safety
	Check
	Yes
	No

	No evidence of structural movement
	□
	□

	Ceilings sound
	□
	□

	Walls stable
	□
	□

	No loose external elements
	□
	□



SECTION 3
HHSRS PHYSIOLOGICAL HAZARDS
Excess Cold
	Check
	Yes
	No

	Fixed heating system provided
	□
	□

	Heating operational
	□
	□

	Tenant reports adequate warmth
	□
	□

	Windows and doors reasonably draught proof
	□
	□


Damp & Mould
	Check
	Yes
	No

	No visible mould growth
	□
	□

	No signs of penetrating damp
	□
	□

	No signs of rising damp
	□
	□

	Adequate ventilation provided
	□
	□

	Extract fans operational
	□
	□


Excess Heat
	Check
	Yes
	No

	Adequate ventilation available
	□
	□

	Windows open safely
	□
	□

	Cooling opportunities available
	□
	□


Indoor Air Quality
	Check
	Yes
	No

	No strong odours
	□
	□

	Ventilation adequate
	□
	□

	No obvious pollutants
	□
	□


Water Supply
	Check
	Yes
	No

	Hot water available
	□
	□

	Water pressure satisfactory
	□
	□

	No leaks visible
	□
	□



SECTION 4
HHSRS INFECTION & HYGIENE HAZARDS
Kitchen Facilities
	Check
	Yes
	No

	Facilities clean and serviceable
	□
	□

	Food preparation areas suitable
	□
	□

	Waste disposal arrangements adequate
	□
	□


Bathrooms
	Check
	Yes
	No

	Sanitary facilities functional
	□
	□

	No leaks
	□
	□

	Ventilation adequate
	□
	□

	No mould present
	□
	□



SECTION 5
HHSRS PSYCHOLOGICAL HAZARDS
Security
	Check
	Yes
	No

	Front door secure
	□
	□

	Window locks functioning
	□
	□

	External lighting adequate
	□
	□


Lighting
	Check
	Yes
	No

	Natural light adequate
	□
	□

	Artificial lighting adequate
	□
	□


Noise
	Check
	Yes
	No

	Excessive noise concerns reported
	□
	□

	Noise mitigation measures present where appropriate
	□
	□


Crowding & Space
	Check
	Yes
	No

	Occupancy appropriate
	□
	□

	Rooms suitable for intended use
	□
	□



SECTION 6
TENANT FEEDBACK
Any concerns raised by the tenant?




SECTION 7
ACTION PLAN
	Issue Identified
	Priority
	Action Required
	Target Date

	
	High / Medium / Low
	
	

	
	High / Medium / Low
	
	

	
	High / Medium / Low
	
	



SECTION 8
INSPECTOR SUMMARY
Overall Property Condition
□ Excellent
□ Good
□ Satisfactory
□ Improvement Required
□ Urgent Action Required
Inspection Summary



Inspector Signature:

Date:


EMPO BEST PRACTICE GUIDANCE
When carrying out inspections:
✓ Take photographs of all rooms
✓ Record any defects immediately
✓ Investigate any reports of damp or mould
✓ Test smoke alarms where possible
✓ Check handrails and stair safety
✓ Ask tenants about heating and ventilation
✓ Record all actions arising from the inspection
✓ Retain inspection records for a minimum of six years
Remember:
The purpose of an inspection is not simply to identify repairs. It is to identify anything that could affect the health, safety or wellbeing of occupants and to take reasonable steps to address those risks before they become hazards.
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